<wap-provisioningdoc> 
    <characteristic type="Metabase">
        <characteristic type="Registry\HKCR\*">
            <parm name="rw-access" value="3"/>
            <parm name="access-role" value="24"/>
        </characteristic>
    </characteristic>
	<!-- ==================Settings -> LightDetectOn =================== -->
    <characteristic type="Metabase">
        <characteristic type="Registry\HKCU\ControlPanel\Backlight\LightDetectOn">
            <parm name="datatype" value="integer"/>
            <parm name="maxvalue" value="10" />
            <parm name="minvalue" value="0" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="label">
                <parm name="0404" value="鍵盤感光模式:"/>
                <parm name="0406" value="Aktiver lysføler:"/>
                <parm name="0407" value="Lichtsensor aktivieren:"/>
                <parm name="0409" value="Light Sensor Enable:"/>
                <parm name="040C" value="Détecteur Lumière activé:"/>
                <parm name="040E" value="Fényérzékelő engedélyezése:"/>
                <parm name="0410" value="Abilita sensore luce:"/>
                <parm name="0413" value="Lichtsensor ingeschakeld:"/>
                <parm name="0418" value="Senzor lumină:"/>
                <parm name="0419" value="Включить световой сенсор:"/>
                <parm name="0804" value="键盘感光模式:"/>
                <parm name="0809" value="Light Sensor Enable:"/>
                <parm name="0C0A" value="Habilitar sensor luminoso:"/>
            </characteristic>
            <characteristic type="options">
                <parm name="0404" value="啟用&#xF001;1&#xF000; 關閉&#xF001;0" />
                <parm name="0406" value="Til&#xF001;1&#xF000;Fra&#xF001;0" />
                <parm name="0407" value="Ein&#xF001;1&#xF000;Aus&#xF001;0" />
                <parm name="0409" value="On&#xF001;1&#xF000;Off&#xF001;0" />
                <parm name="040C" value="Actif&#xF001;1&#xF000;Inactif&#xF001;0" />
                <parm name="040E" value="Be&#xF001;1&#xF000;Ki&#xF001;0" />
                <parm name="0410" value="On&#xF001;1&#xF000;Off&#xF001;0" />
                <parm name="0413" value="Aan&#xF001;1&#xF000;Uit&#xF001;0" />
                <parm name="0418" value="Pornit&#xF001;1&#xF000;Oprit&#xF001;0" />
                <parm name="0419" value="вкл&#xF001;1&#xF000;выкл&#xF001;0" />
                <parm name="0804" value="打开&#xF001;1&#xF000; 关闭&#xF001;0" />
                <parm name="0809" value="On&#xF001;1&#xF000;Off&#xF001;0" />
                <parm name="0C0A" value="Encendido&#xF001;1&#xF000;Apagado&#xF001;0" />
            </characteristic>
        </characteristic>
	</characteristic>
	<!-- ==================Settings -> Photo Sensor On =================== -->
    <characteristic type="Metabase">
        <characteristic type="Registry\HKCU\ControlPanel\Backlight\PhotoSensorOn">
            <parm name="datatype" value="integer"/>
            <parm name="maxvalue" value="1" />
            <parm name="minvalue" value="0" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="label">
                <parm name="0409" value="Backlight Mode:"/>
            </characteristic>
            <characteristic type="options">
                <parm name="0409" value="Auto&#xF001;1&#xF000;Manual&#xF001;0" />
            </characteristic>
        </characteristic>
	</characteristic>
	<!-- ==================Settings -> Backlight Level =================== -->
    <characteristic type="Metabase">
        <characteristic type="Registry\HKCU\ControlPanel\Backlight\BacklightLevel">
            <parm name="datatype" value="integer"/>
            <parm name="maxvalue" value="3" />
            <parm name="minvalue" value="1" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="label">
                <parm name="0409" value="Backlight Brightness:"/>
            </characteristic>
            <characteristic type="options">
                <parm name="0409" value="1&#xF001;1&#xF000;2&#xF001;0" />
            </characteristic>
        </characteristic>
	</characteristic>
	<!-- ==================Settings -> CSD Type =================== -->
     <characteristic type="Metabase">
        <characteristic type="Registry\HKCU\ControlPanel\PhoneExtendFunction\CBSTSpeed">
            <parm name="datatype" value="integer"/>
            <parm name="maxvalue" value="71" />
            <parm name="minvalue" value="7" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="label">
                <parm name="0404" value="資料傳輸率:"/>
                <parm name="0405" value="Rychlost pøenosu dat: "/>
                <parm name="0406" value="Datahastighed: "/>
                <parm name="0407" value="Datenrate: "/>
                <parm name="0408" value="Ρυθμός μεταφοράς:"/>
                <parm name="0409" value="Data rate:"/>
                <parm name="040B" value="Datanopeus:"/>
                <parm name="040C" value="Débit: "/>
                <parm name="040E" value="Adatsebesség:"/>
                <parm name="0410" value="Velocità dati:"/>
                <parm name="0413" value="Gegevenssnelheid:"/>
                <parm name="0414" value="Datatakt:"/>
                <parm name="0415" value="Szybkość transmisji danych: "/>
                <parm name="0418" value="Ratã date: "/>
                <parm name="0419" value="Скорость передачи данных:"/>
                <parm name="041B" value="Rýchlosť prenosu dát: "/>
                <parm name="041D" value="Datafrekvens:"/>
                <parm name="041F" value="Veri hızı: "/>
                <parm name="0804" value="速率:"/>
                <parm name="0816" value="Taxa de dados: "/>
                <parm name="0C0A" value="Velocidad de datos: "/>
                <parm name="0416" value="Taxa de dados:"/>
            </characteristic>
            <characteristic type="options">
                   <parm name="0409" value="9600 bps(v.32)&#xF001;7&#xF000;9600 bps(v.110)&#xF001;71&#xF000;9600 bps(v.34)&#xF001;12" />
            </characteristic>
        </characteristic>    
    </characteristic>
    <characteristic type="Metabase">
        <characteristic type="Registry\HKCU\ControlPanel\PhoneExtendFunction\CBSTCe">
            <parm name="datatype" value="integer"/>
            <parm name="maxvalue" value="1" />
            <parm name="minvalue" value="0" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="label">
                <parm name="0404" value="連接元件:"/>
                <parm name="0405" value=" Spojovací prvek:"/>
                <parm name="0406" value="Tilslutningselement: "/>
                <parm name="0407" value="Verbindungselement:"/>
                <parm name="0408" value="Στοιχείο σύνδεσης:"/>
                <parm name="0409" value="Connection element:"/>
                <parm name="040B" value="Yhteyselementti:"/>
                <parm name="040C" value="Element de connexion:"/>
                <parm name="040E" value="Összeköttetés-elem:"/>
                <parm name="0410" value="Elemento di connessione:"/>
                <parm name="0413" value="Verbindingselement:"/>
                <parm name="0414" value="Tilkoblingselement:"/>
                <parm name="0415" value="Element połączenia: "/>
                <parm name="0418" value="Element conexiune: "/>
                <parm name="0419" value="Элемент подключения:"/>
                <parm name="041B" value="Spojovací prvok: "/>
                <parm name="041D" value="Anslutningselement:"/>
                <parm name="041F" value="Bağlantı elemanı: "/>
                <parm name="0804" value="连接元素:"/>
                <parm name="0816" value="Elemento de conexão: "/>
                <parm name="0C0A" value="Elemento de conexión: "/>
                <parm name="0416" value="Elemento de conexão:"/>
            </characteristic>
            <characteristic type="options">
                <parm name="0404" value="透明&#xF001;0&#xF000;非透明&#xF001;1" />
                <parm name="0405" value=" Transparentní&#xF001;0&#xF000;Netransparentní &#xF001;1" />
                <parm name="0406" value="Gennemsigtig&#xF001;0&#xF000;Ikke-gennemsigtig &#xF001;1" />
                <parm name="0407" value="Transparent &#xF001;0&#xF000;Nicht transparent &#xF001;1" />
                <parm name="0408" value="Διαφανής&#xF001;0&#xF000;Μη διαφανής&#xF001;1" />
                <parm name="0409" value="Transparent&#xF001;0&#xF000;Non-transparent&#xF001;1" />
                <parm name="040B" value="Läpinäkyvä&#xF001;0&#xF000;Läpinäkymätön&#xF001;1" />
                <parm name="040C" value="Transparent&#xF001;0&#xF000;Non transparent &#xF001;1" />
                <parm name="040E" value="Transzparens &#xF001;0&#xF000;Nem transzparens &#xF001;1" />
                <parm name="0410" value="Assente &#xF001;0&#xF000;Non-assente &#xF001;1" />
                <parm name="0413" value="Transparant&#xF001;0&#xF000;Niet transparant&#xF001;1" />
                <parm name="0414" value="Gjennomsiktig&#xF001;0&#xF000;Ikke-gjennomsiktig&#xF001;1" />
                <parm name="0415" value="Przezroczysty &#xF001;0&#xF000;Nieprzezroczysty &#xF001;1" />
                <parm name="0418" value="Transparent &#xF001;0&#xF000;Ne-transparent &#xF001;1" />
                <parm name="0419" value="Прозрачный&#xF001;0&#xF000; Непрозрачный&#xF001;1" />
                <parm name="041B" value="Priehľadný &#xF001;0&#xF000;Nepriehľadný &#xF001;1" />
                <parm name="041D" value="Genomskinlig&#xF001;0&#xF000;Ogenomskinlig&#xF001;1" />
                <parm name="041F" value="Saydam &#xF001;0&#xF000;Saydam olmayan &#xF001;1" />
                <parm name="0804" value="透明的&#xF001;0&#xF000;非透明的&#xF001;1" />
                <parm name="0816" value="Transparente &#xF001;0&#xF000;Não-transparente &#xF001;1" />
                <parm name="0C0A" value="Transparente &#xF001;0&#xF000;No transparente &#xF001;1" />
                <parm name="0416" value="Transparente &#xF001;0&#xF000;Não-transparente &#xF001;1" />
            </characteristic>
        </characteristic>    
    </characteristic>
    <characteristic type="Metabase">
        <characteristic type="Registry\HKCU\ControlPanel\PhoneExtendFunction\CBSTName" >
            <parm name="datatype" value="integer"/>
            <parm name="semantic-type" value="invisible"/>
            <parm name="maxvalue" value="1" />
            <parm name="minvalue" value="0" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="options">
                 <parm name="0409" value="0 &#xF001;0" />
             </characteristic>
        </characteristic>
    </characteristic>
	<!-- ==================Settings -> Bluetooth Device Name =================== -->
     <characteristic type="Metabase">
        <characteristic type="HTCCSP\BluetoothDeviceName">
            <parm name="datatype" value="string"/>
            <parm name="maxlength" value="32"/>
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="label">
                <parm name="0404" value="裝置名稱:"/>
                <parm name="0405" value="Název zařízení:"/>
                <parm name="0406" value="Enhedsnavn:"/>
                <parm name="0407" value="Gerätename:"/>
                <parm name="0408" value="Όνομα συσκευής:"/>
                <parm name="0409" value="Device name:"/>
                <parm name="040B" value="Laitteen nimi:"/>
                <parm name="040C" value="Nom d'appareil :"/>
                <parm name="040E" value="Eszköznév:"/>
                <parm name="0410" value="Nome dispositivo:"/>
                <parm name="0413" value="Apparaatnaam:"/>
                <parm name="0414" value="Enhetsnavn:"/>
                <parm name="0415" value="Nazwa urządzenia:"/>
                <parm name="0416" value="Nome do dispositivo:"/>
                <parm name="0418" value="Nume dispozitiv:"/>
                <parm name="0419" value="Имя устройства:"/>
                <parm name="041B" value="Názov zariadenia:"/>
                <parm name="041D" value="Enhetsnamn:"/>
                <parm name="041F" value="Aygıt Adı:"/>
                <parm name="0804" value="设备名称:"/>
                <parm name="0816" value="Nome de dispositivo:"/>
                <parm name="0C0A" value="Nombre de dispositivo:"/>
            </characteristic>
        </characteristic>    
    </characteristic>
	<!-- ==================Settings -> Bluetooth Beam Authentication =================== -->
     <characteristic type="Metabase">
        <characteristic type="Registry\HKLM\SOFTWARE\Microsoft\Obex\Services\{00000000-0000-0000-0000-000000000000}\TransportAuthenticate">
            <parm name="datatype" value="boolean"/>
            <parm name="maxvalue" value="1" />
            <parm name="minvalue" value="0" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />
            <characteristic type="label">
                <parm name="0404" value="OBEX需要認證(密碼)"/>
                <parm name="0405" value="Je vyžadováno ověření OBEX (heslo)."/>
                <parm name="0406" value="OBEX-godkendelse (adgangskode) kræves."/>
                <parm name="0407" value="OBEX-Authentifizierung (Kennwort) erforderlich."/>
                <parm name="0408" value="Απαιτείται επικύρωση (κωδικός) OBEX."/>
                <parm name="0409" value="OBEX authentication(Passkey) required."/>
                <parm name="040B" value="OBEX-tunnistus (yleisavain) vaaditaan."/>
                <parm name="040C" value="Authentification OBEX (passe) requise :"/>
                <parm name="040E" value="OBEX hitelesítés (jelkulcs) szükséges."/>
                <parm name="0410" value="Autenticazione OBEX (Password) richiesta."/>
                <parm name="0413" value="OBEX-waarmerking (passkey) vereist."/>
                <parm name="0414" value="OBEX-autentisering (passord) nødvendig."/>
                <parm name="0415" value="Wymagane uwierzytelnianie OBEX (Hasło)."/>
                <parm name="0416" value="Autenticação OBEX (chave de acesso) necessária."/>
                <parm name="0418" value="Este necesară autentificare OBEX (Passkey)."/>
                <parm name="0419" value="Требуется аутентификация OBEX (пароль)."/>
                <parm name="041B" value="Vyžaduje sa overenie OBEX (Passkey)"/>
                <parm name="041D" value="OBEX-autentisering (lösenord) krävs."/>
                <parm name="041F" value="OBEX Kimlik Denetimi (Geçiş Anahtarı) gerekli."/>
                <parm name="0804" value="需 OBEX 身份鉴定 (密码)。

"/>
                <parm name="0816" value="Autenticação OBEX (palavra-chave) necessária."/>
                <parm name="0C0A" value="Autenticación OBEX (clave de paso) requerida."/>
            </characteristic>
        </characteristic>    
    </characteristic>
<!--====================== wap push mail ====================-->   
    <characteristic type="Metabase">
        <characteristic type="Registry\HKLM\Security\Policies\Policies\00001011">
            <parm name="datatype" value="integer"/>
            <parm name="maxvalue" value="1" />
            <parm name="minvalue" value="0" />
            <parm name="rw-access" value="3" />
            <parm name="access-role" value="190" />

            <characteristic type="label">
			<parm name="0409" value="WAP Push Message: "/>
			<parm name="0404" value="WAP Push 訊息: "/>
			<parm name="0405" value="Zpráva WAP Push: "/>
			<parm name="0406" value="WAP skub meddelelse: "/>
			<parm name="0407" value="WAP-Push-Nachricht: "/>
			<parm name="0410" value="Messaggio WAP Push: "/>
			<parm name="0413" value="WAP Push-bericht: "/>
			<parm name="0414" value="WAP-pushmelding: "/>
			<parm name="0415" value="Wiadomość WAP typu push: "/>
			<parm name="0416" value="Mensagem push WAP: "/>
			<parm name="0419" value="Сообщение WAP Push: "/>
			<parm name="040b" value="WAP Push-viesti: "/>
			<parm name="040c" value="Message WAP Push: "/>
			<parm name="041d" value="WAP push-meddelande: "/>
			<parm name="0408" value="Ωθούμενο μήνυμα WAP: "/>
			<parm name="040E" value="WAP küldési üzenet: "/>
			<parm name="0418" value="Retransmitere mesaj WAP: "/>
			<parm name="041b" value="Push správa cez WAP: "/>
			<parm name="041f" value="WAP Push Mesajı: "/>
			<parm name="0c0a" value="Mensaje push WAP: "/>
			<parm name="0816" value="Mensagem WAP Push: "/>
			<parm name="0804" value="WAP 推送信息: "/>
            </characteristic>

            <characteristic type="options">
			<parm name="0409" value="Disable&#xF001;0&#xF000;Enable&#xF001;1" />
			<parm name="0804" value="禁用&#xF001;0&#xF000;启用&#xF001;1" />
			<parm name="0404" value="停用&#xF001;0&#xF000;啟用&#xF001;1" />
			<parm name="0405" value="zakázáno&#xF001;0&#xF000;povoleno&#xF001;1" />
			<parm name="0406" value="deaktiveret&#xF001;0&#xF000;aktiveret&#xF001;1" />
			<parm name="040C" value="désactivé&#xF001;0&#xF000;activé&#xF001;1" />
			<parm name="0407" value="deaktiviert&#xF001;0&#xF000;aktiviert&#xF001;1" />
			<parm name="040E" value="letiltva&#xF001;0&#xF000;engedélyezve&#xF001;1" />
			<parm name="0410" value="disabilitato&#xF001;0&#xF000;abilitato&#xF001;1" />
			<parm name="0415" value="wyłączone&#xF001;0&#xF000;włączone&#xF001;1" />
			<parm name="0816" value="desactivado&#xF001;0&#xF000;activado&#xF001;1" />
			<parm name="0418" value="dezactivat&#xF001;0&#xF000;activat&#xF001;1" />
			<parm name="041B" value="zakázané&#xF001;0&#xF000;povolené&#xF001;1" />
			<parm name="0C0A" value="deshabilitado&#xF001;0&#xF000;habilitado&#xF001;1" />
			<parm name="041F" value="devre dışı&#xF001;0&#xF000;etkin&#xF001;1" />
			<parm name="0413" value="uitgeschakeld&#xF001;0&#xF000;ingeschakeld&#xF001;1" />
			<parm name="0419" value="отключена&#xF001;0&#xF000;включена&#xF001;1" />
			<parm name="041D" value="inaktiverad&#xF001;0&#xF000;aktiverad&#xF001;1" />
			<parm name="0414" value="deaktivert&#xF001;0&#xF000;aktivert&#xF001;1" />
			<parm name="040B" value="ei käytössä&#xF001;0&#xF000;käytössä&#xF001;1" />
			<parm name="0408" value="απενεργοποιήθηκε&#xF001;0&#xF000; ενεργοποιημένο&#xF001;1" />
			<parm name="0416" value="Desabilitar&#xF001;0&#xF000;Habilitar&#xF001;1" />
            </characteristic>
        </characteristic>
    </characteristic>
	
	<characteristic type="Registry">
	  <characteristic type="HKLM\Platform" >
		 <parm name="OEM_100_PROVXML" value="1" datatype="integer" />
	  </characteristic>        
	</characteristic>   
</wap-provisioningdoc>
