<wap-provisioningdoc>

	<characteristic type="SecurityPolicy">
	<!--3716 adds 512, Trusted PPG, default is 3204 -->
        <!--  20080411 ITS: 233 Set 4119 from 132(Default) to 132+32=164  -->        
		<parm name="4119" value="164"/>
		<parm name="4141" value="4096"/>
		<parm name="4142" value="3712"/>
		<parm name="4143" value="4096"/>
        <!-- Service Loading Policy-->
        <!-- PPG_TRUSTED|SECROLE_OPERATOR-->
<!-- Fix DIAMOND_C ITS 2322 According to RIL/Fangling_Chuangrequest -->             
		<parm name="4108" value="2244"/>
        <!-- Service Indication Policy-->
        <!-- PPG_AUTH | PPG_TRUSTED|SECROLE_OPERATOR-->
		<parm name="4109" value="3268"/>
        <!-- SL Security Policy -->
        <!-- use http or wap-->
		<parm name="4124" value="1"/>
	</characteristic>
		
<characteristic type="Registry">
	<!-- **********************************Region Setting*************************************** -->
	<characteristic type="HKLM\nls" translation="filesystem">
	  	<parm name="DefaultLCID" datatype="integer" value="4105" translation="filesystem"/>
	</characteristic>
	<!--20071031, DST new solution by ITS 1717 -->
	<characteristic type="HKLM\SOFTWARE\Microsoft\Clock">
    		<parm name="Home" datatype="integer" value="290"/>
  	</characteristic>

    <!-- ============================ System: ##Menu ================================= -->
	<characteristic type="HKLM\Services\PhoneExt\KeyProgram" translation="filesystem">
			<parm name="Prefix" datatype="string" value="#" translation="filesystem"/>
			<parm name="Postfix" datatype="string" value="#" translation="filesystem"/>	<!--2007-05-31, Cutsomer's ITS.9853,add ##menu#,from shenhow -->
			<parm name="Prog0" datatype="string" value="EPST.exe ##778" translation="filesystem"/>
			<parm name="Key0" datatype="string" value="#778" translation="filesystem"/>
			<parm name="Prog1" datatype="string" value="FieldTrial.exe" translation="filesystem"/>
			<parm name="Key1" datatype="string" value="#33284" translation="filesystem"/>
			<parm name="Prog2" datatype="string" value="DMRouter.exe /OPEN_MODEM_PORT"/>
			<parm name="Key2" datatype="string" value="#3424" translation="filesystem"/>
			<parm name="Prog4" datatype="string" value="EPST.exe ##775" translation="filesystem"/>
			<parm name="Key4" datatype="string" value="#775" translation="filesystem"/>
 			<parm name="Prog5" datatype="string" value="Fuart.exe FSUSB" translation="filesystem"/>
			<parm name="Key5" datatype="string" value="#37872" translation="filesystem"/>
			<parm name="Prog6" datatype="string" value="EPST.exe ##786" translation="filesystem"/>
			<parm name="Key6" datatype="string" value="#786" translation="filesystem"/>
	</characteristic>
<!-- Hermann#C ITS#1568: [AP2:DM][BM]It will start VA session right after entering "*723" (without pressing "send") -->
	<characteristic type="HKCU\ControlPanel\PhoneExtendFunction\CDMA"  translation="filesystem" >
		<parm name="EnableOMADMClient" datatype="integer" value="1" />
	</characteristic>
	<characteristic type="HKLM\Services\PhoneExt\KeyProgramExt"  translation="filesystem" >
		<parm name="OMADMClientKey" datatype="string" value="*723"  translation="filesystem"  />
	</characteristic>
		
	<!-- According to SWPM request, add below information -->
	<!-- ##DM_router, Create a short cut DM_router.exe with Parameter "/OPEN_MODEM_PORT", DMRouter will launch DIAG UI and open the modem port.-->
	<characteristic type="HKLM\Software\OEM\DMRouter" translation="filesystem">
		<parm name="ModemPortName" datatype="string" value="COM8:" translation="filesystem"/>
	</characteristic>
    
    <!-- ============================ System: Phone settings ================================= -->
        <!-- 5-2 Other Phone settings -->
    	<!-- Network Service -->
	<characteristic type="HKLM\SOFTWARE\OEM\InitProv\PhoneSetting" translation="filesystem">
		<parm name="ServiceName" datatype="string" value="Network Service" translation="filesystem"/>
		<parm name="ServiceTitle" datatype="string" value="Phone: Preferred Serving System" translation="filesystem"/>
		<parm name="ItemCount" datatype="integer" value="2"/>
		<parm name="ItemName1" datatype="string" value="Home only" translation="filesystem"/>
		<parm name="ItemValue1" datatype="integer" value="1"/>
		<parm name="ItemName2" datatype="string" value="Standard" translation="filesystem"/>
		<parm name="ItemValue2" datatype="integer" value="4"/>
	</characteristic>
	<characteristic type="HKLM\Software\OEM\PhoneSetting\NetworkService"  translation="filesystem" >
		<parm name="ServiceName" datatype="string" value="Preferred Serving System"  translation="filesystem"  />
	</characteristic>
    	<!-- LocationSetting -->		
	<characteristic type="HKLM\SOFTWARE\OEM\PhoneSetting\LocationSetting"  translation="filesystem" >
		<parm name="ServiceName" datatype="string" value="Location Setting"  translation="filesystem"  />
		<parm name="ServiceTitle" datatype="string" value="Phone: Location Setting"  translation="filesystem"  />
		<parm name="ServiceDesc" datatype="string" value="Turning location &#x22;ON&#x22; lets the network detect your geographic location using GPS, making some features easier to use. "  translation="filesystem"  />
		<parm name="ServiceDescExt" datatype="string" value="Turning location &#x22;OFF&#x22; disables GPS, but some features may still detect your whereabouts using cell tower technology. Except for basic telephone and 911 service, your location information will only be used with your consent. "  translation="filesystem"  />
		<parm name="ItemCount" datatype="integer" value="2" />
		<parm name="ItemName1" datatype="string" value="ON"  translation="filesystem"  />
		<parm name="ItemValue1" datatype="integer" value="0" />
		<parm name="ItemMessageDesc1" datatype="string" value="Turning location &#x22;ON&#x22; lets the network detect your whereabouts using GPS"  translation="filesystem"  />
		<parm name="ItemName2" datatype="string" value="OFF"  translation="filesystem"  />
		<parm name="ItemValue2" datatype="integer" value="3" />
		<parm name="ItemMessageDesc2" datatype="string" value="Turning location &#x22;OFF&#x22; disables GPS - except for 911 - but cell tower technology may still be used to detect your whereabouts for some features and basic telephone service."  translation="filesystem"  />
	</characteristic>
	<!-- TtyMode -->
	<!-- According to SWPM request, update below information, NEON_C ITS 130 20080507-->
	<!--
             [HKEY_LOCAL_MACHINE\Software\OEM\PhoneSetting\TtyMode]
             "ItemValue1" = dword:00000001 (on:1)
             "ItemValue2" = dword:00000000 (off: 0)
         -->
         
         
		<!-- TtyMode -->
				
		<characteristic type="HKLM\SOFTWARE\OEM\PhoneSetting\TtyMode" translation="filesystem">
			<parm name="ServiceName" datatype="string" value="TTY Mode" translation="filesystem"/>
			<parm name="ServiceTitle" datatype="string" value="Phone: TTY Mode" translation="filesystem"/>
			<parm name="ItemCount" datatype="integer" value="4"/>
			<parm name="ItemName1" datatype="string" value="Full mode" translation="filesystem"/>
			<parm name="ItemValue1" datatype="integer" value="1"/>
			<parm name="ItemName2" datatype="string" value="VCO mode" translation="filesystem"/>
			<parm name="ItemValue2" datatype="integer" value="2"/>
			<parm name="ItemName3" datatype="string" value="HCO mode" translation="filesystem"/>
			<parm name="ItemValue3" datatype="integer" value="3"/>
			<parm name="ItemName4" datatype="string" value="Off" translation="filesystem"/>
			<parm name="ItemValue4" datatype="integer" value="0"/>
		</characteristic>

		
	<!--   Enable registry of TTY in the Phonesetting  -->
	<!--(0: 1:vibrate, 2:vibrate and ring, 3:vibrate than ring, 4:notify and ringtone set to vibrate)-->
	<characteristic type="HKCU\ControlPanel\PhoneExtendFunction\CDMA" translation="filesystem">
      		<parm name="Tty_Mode_Vibrate" datatype="integer" value="4" translation="filesystem"/>
	</characteristic>
	  

	  
	<!-- *************************Hidden PhoneSetting***************************** -->
	<characteristic type="HKCU\ControlPanel\PhoneExtendFunction\CDMA" translation="filesystem">
		<parm name="CallForward" datatype="integer" value="0"/>
		<parm name="CallWait" datatype="integer" value="0"/>
		<parm name="SMS" datatype="integer" value="0"/>
		<parm name="Internet" datatype="integer" value="0"/>
		<parm name="Bcsms" datatype="integer" value="0"/>
	</characteristic>

	<characteristic type="HKLM\Software\OEM\PhoneSetting" translation="filesystem">
		<parm name="HiddenDeleteVM" datatype="integer" value="0" translation="filesystem"/>
		<parm name="HiddenPreferenceMode" datatype="integer" value="0" translation="filesystem"/>
		<parm name="HiddenTimesyncPage" datatype="integer" value="0" translation="filesystem"/>
		<parm name="HiddenAlertPage" datatype="integer" value="1" translation="filesystem"/>
		<parm name="HiddenNAMSelectPage" datatype="integer" value="1" translation="filesystem"/>
		<parm name="HiddenVoicePrivacyPage" datatype="integer" value="1" translation="filesystem"/>
		<parm name="HiddenModeOperationPage" datatype="integer" value="0" translation="filesystem"/>
		<parm name="HiddenPlusCodeDialingPage" datatype="integer" value="1" translation="filesystem"/>
		<parm name="ShowAutoPrependPage" datatype="integer" value="1" />
		<parm name="AutoPrepend_1" datatype="integer" value="0" /><!--ITS.802,AutoPrepend default setting should be disable -->
	</characteristic>
		

	<!--  (1       : enable NITZ function)    (0, none : disable NITZ function) -->
	 <characteristic type="HKLM\Drivers\BuiltIn\RIL" translation="filesystem">
		<parm name="NITZEnable" datatype="integer" value="1" translation="filesystem"/>
	</characteristic>
	
	<!--Home Only -->
	<characteristic type="HKLM\Services\PhoneExt" translation="filesystem">
		<parm name="ShowHomeOnly" datatype="integer" value="1" translation="filesystem"/>
	</characteristic>


	
<!-- ============================ System: Text Messaging (SMS) ================================= -->			
	<!--SMS Timestamp enable	-->
	 <characteristic type="HKLM\Software\OEM\SMS" translation="filesystem">
	  	<parm name="RecvTimeStamp" datatype="integer" value="1" translation="filesystem"/>
	 </characteristic>
		
	<!--    Network SMSDeliveryNotify  -->
	<characteristic type="HKCU\Software\Microsoft\Inbox\Settings" translation="filesystem">
		<parm name="SMSDeliveryNotify" datatype="integer" value="0" translation="filesystem"/>
	</characteristic>
		
	<!--SMSInteractive-->
 	<characteristic type="HKLM\Software\OEM\SMS" translation="filesystem">
  		<parm name="InteractiveMTSmsToNormal" datatype="integer" value="1" translation="filesystem"/>
   	</characteristic>

 	<!--SMSPriority-->
	 <characteristic type="HKLM\Software\OEM\SMS" translation="filesystem">
		<parm name="PriorityHighLevel" datatype="integer" value="2" translation="filesystem"/>
	 	<parm name="EnablePriorityHighLevel" datatype="integer" value="1" translation="filesystem"/>
	</characteristic>
	 
	 <!-- Configuring the SMS Message Character Limit -->
	<characteristic type="HKCU\Software\Microsoft\SMS\TextShared"  translation="filesystem" >
		<parm name="IS637MaxAsciiCharacters" datatype="integer" value="140" />
    	</characteristic>
	 	 
<!--   8BIT_UNICODE -->
<!-- 	1,  7BIT_ONLY
        2,  7BIT  + UNICODE
	3,  8BIT_ONLY
	4,  8BIT + UNICODE
--> 
<!-- 2008/9/18, requested by Henry Cheng  10:52 AM set MSGType=2 -->
<!-- Fix ITS4016 [Bell Mobility][[BM_Victor]14669][N/A]SMS: French SMS greater than 70 characters are sent as 2 data bursts -->
	<characteristic type="HKCU\ControlPanel\PhoneExtendFunction\CDMA"  translation="filesystem" >
		<parm name="MsgType" datatype="integer" value="2" />
	</characteristic>
	<characteristic type="HKLM\SOFTWARE\OEM\RILCUST\BM\ExtendSMSLen"  translation="filesystem" >
		<parm name="Enabled" datatype="integer" value="1" />
	</characteristic>		
<!-- ============================ Others ================================= -->	
    	<!-- Set EV ICON.-->
    	<!--
  	<characteristic type="HKLM\Security\ResOver\Bitmaps" translation="filesystem">
   		<parm name="BaseDll" datatype="string" value="Override_BM.dll" translation="filesystem"/>
  	</characteristic>
  	-->
  	
  	<!--  Error code setting  -->
  	<characteristic type="HKLM\Services\PhoneExt\DataFailCode" translation="filesystem">
		  <parm name="36" datatype="string" value="Error Code 36     Misc error setting up Simple IP" translation="filesystem"/>
		  <parm name="37" datatype="string" value="Error Code 37     Misc error setting up Mobile IP" translation="filesystem"/>
	</characteristic>
  			
	<!-- ******************************Commom Setting******************************-->
	<!--Button Lock-->
	<characteristic type="HKLM\HARDWARE\OEM\KEYBD" translation="filesystem">
		<parm name="KeyLock" datatype="integer" value="1"/>
	</characteristic>
		
	<characteristic type="HKLM\SOFTWARE\OEM\FieldTrial" translation="filesystem">
		<parm name="DisablePage" datatype="integer" value="4"/>
	</characteristic>

   	<!-- According to Shenhow request, BM and Sprint to show Ecall in the call history.(Titan and Libra)  -->
   	<!-- While this registry is set to 1, all the ECC numbers read from radio save to No-log registry.
        Otherwise, CE will not save radio ECC numbers to No-log(for Sprint). -->
	<characteristic type="HKLM\Security\Phone\NoLog" translation="filesystem">
		<parm name="EnableRadioNoLog" datatype="integer" value="0" />
		<parm name="List" value="" datatype="multiplestring" translation="filesystem"/>
	</characteristic>


	<!-- According to SWPM request, add below information -->
	<!-- 04/17/2007 ITS.2533  [BM] Fail to send the French SMS, no MOSMSUseLatinEncode DWord key in this build. 
	-->	
	<!--French SMS set the registry.  -->
	<characteristic type="HKLM\System\Inbox\Settings" translation="filesystem">
		<parm name="MOSMSUseLatinEncode" datatype="integer" value="1" />
	</characteristic>
		
	<!-- 05/28/2007 ITS2679  [Bell Mobility][VAS Feature][[BM]10269][N/A]SMS: Handset does not inform the user about message sending failure due to unknown destination address -->
	<characteristic type="HKCU\ControlPanel\PhoneExtendFunction\CDMA" translation="filesystem">
  	         <parm name="PhoneExt_SmsRetry" datatype="integer" value="1" />
    	</characteristic>
    
    	<!-- 05/28/2007 Enable item "BT IP Address" -->
	<characteristic type="HKLM\SOFTWARE\OEM\DIM" translation="filesystem">
  	         <parm name="EnableBTIPAddress" datatype="integer" value="1" />
    	</characteristic>

	<!-- 05/29/2007 Now this item string only support for ENG Ver. BT Core spec version read from: -->
	<characteristic type="HKLM\software\OEM" translation="filesystem">
  	         <parm name="CoreSpecVer" datatype="string" value="2.0/2.0+EDR"   translation="filesystem" />
         </characteristic>

	<!--2007/6/12, per SWPM's request, Add a registry to disable the "Error Class: and Cause Code:" in the SMS retry message.
	[HKEY_LOCAL_MACHINE\Services\PhoneExt]
	"SMSRetryType"=dword:00000001
	(the default value is 0) 
	If the SMSRetryType = 0, it will show the "Error Class: and Cause Code:" in the SMS retry bubble message. 
	If the SMSRetryType = 1, it will not show the "Error Class: and Cause Code:" in the SMS retry bubble message. 
	-->
 	<characteristic type="HKLM\Services\PhoneExt"  translation="filesystem" >
   		<parm name="SMSRetryType" datatype="integer" value="1"/>
 	</characteristic>

	<!--20070726,add sounds for Phone ON and Off -->
	<characteristic type="HKCU\ControlPanel\PhoneExtendFunction\CDMA\FlightModeOnOFF" translation="filesystem">
			<parm name="EnableSound" datatype="integer" value="1" translation="filesystem"/>
			<parm name="Sound_on" datatype="string" value="\windows\PhoneOn.wav" translation="filesystem"/>
			<parm name="Sound_off" datatype="string" value="\windows\PhoneOff.wav" translation="filesystem"/>
	</characteristic>

	<!--2007/8/14, ITS 871,Add M_NAI seting -->
	<characteristic type="HKLM\Comm\InternetSharing">
              <parm name="Extension" value="rilphone.dll" datatype="string"/>
         </characteristic>

	<!--2007/8/14, ITS 980,[BM]SMS Language Indicator attribute in the MO-SMS Data Burst Message shuld not shown as Unknown or unspecified. -->
	<characteristic type="HKLM\Software\OEM\SMS">
              <parm name="Language" value="100" datatype="integer"/>
         </characteristic>
	<!--2008/8/2, Diamond#C ITS 4000-->
	<characteristic type="HKLM\Software\OEM\PhoneSetting"  translation="filesystem" >
		<parm name="HiddenModeOperationPage" datatype="integer" value="0" />
	</characteristic>
	<!--2007/8/15, ITS 983-->
	<characteristic type="HKLM\Software\OEM\PhoneSetting">
              <parm name="EVDOModeMsg" value="1X services will be disabled. Note: The device will be power-cycled to apply the change." datatype="string" translation="filesystem"/>
              <parm name="1XOnlyModeMsg" value="Warning: High speed data calls will be disabled.     Note: The device will be power-cycled to apply the change." datatype="string" translation="filesystem"/>
              <parm name="HybridModeMsg" value="Warning: The device will attempt to connect packet data calls on EVDO and all other attempts to connect to any other type of service will be on 1X." datatype="string" translation="filesystem"/>
         </characteristic>

	<!--2007/8/15,  ITS 984-->
	<characteristic type="HKCU\ControlPanel\PhoneExtendFunction\CDMA">
              	<parm name="EnableIS95DIcon" value="1" datatype="integer"/>
         </characteristic>

	<!--20070814,ITS 985,request by SWPM Jimmy,
	[HKEY_CURRENT_USER\Software\HTC\LongPressEndKey]
	"AutoExecute"=dword:00000000    Prompt (default) 
	"AutoExecute"=dword:00000001    Turn airplane mode on/off (SPCS)
	"AutoExecute"=dword:00000002    Lock device
	"AutoExecute"=dword:00000003    Terminate data connection(Telus/BM)
	"AutoExecute"=dword:00000004    Set Vibrate/Ringer
 	-->
	<characteristic type="HKCU\Software\HTC\LongPressEndKey">
  		<parm name="AutoExecute" datatype="integer" value="3" />
 	</characteristic>

	<!--End of M_NAI -->

	<!--2007/9/26, ITS 1477, add this registry -->
 	<characteristic type="HKLM\Software\OEM\InitProv" translation="filesystem">
   		<parm name="Enable_WriteSMSCallBackNumber" datatype="integer" value="1"/>
 	</characteristic>

	<!--2007/9/28,for WModem, add from ED -->
 	<characteristic type="HKLM\SOFTWARE\OEM\WModem" translation="filesystem">
   		<parm name="PDP" datatype="string" value=""/>
 	</characteristic>

	<!--20071002, SWPM Jack request to add it -->
	<characteristic type="HKLM\SOFTWARE\OEM\WModem"  translation="filesystem" >
			<parm name="Multi-NAI" datatype="integer" value="1" />
	</characteristic>
	<!--20080805, SWPM Henry Cheng requests to add it -->
	<characteristic type="HKLM\SOFTWARE\OEM\WModem"  translation="filesystem" >
		<parm name="Hide Bluetooth" datatype="integer" value="1" />
	</characteristic>
</characteristic>	
</wap-provisioningdoc>
