REGEDIT4

[HKEY_LOCAL_MACHINE\ControlPanel\GPS Settings]
	"Hide"=dword:0
[HKEY_LOCAL_MACHINE\Services\GPSDaemonService]
    "Dll"="GpsDaemonService.dll"
    "DisplayName"="GPS Daemon Service"
    "Description"="Services PPP events on behalf of GPS"
    "Order"=dword:9
    "Keep"=dword:1
    "Prefix" = "GPC"
    "Index"=dword:1
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\GPSID]
   "Dll"="GPSID_QCT.dll"
   "Order"=dword:10
   "Keep"=dword:1
   "Prefix"="GPD"
   "Index"=dword:0
   "Context"=dword:0
   "IClass"="{A32942B7-920C-486b-B0E6-92A702A99B35}"
[HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\Power\State\Unattended]
    "gpd0:"=dword:4
[HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\Power\State\Suspend]
    "gpd0:"=dword:4
[HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\Power\State\Resuming]
    "gpd0:"=dword:4     
[HKEY_LOCAL_MACHINE\System\CurrentControlSet\GPS Intermediate Driver]
        "IsEnabled"=dword:1
        "CurrentLogFile"="\\windows\\GPSLogFile.txt"  
        "OldLogFile"="\\windows\\GPSLogFileBack.txt"
[HKEY_LOCAL_MACHINE\System\CurrentControlSet\GPS Intermediate Driver\Drivers]
    "CurrentDriver"="GPSOneDevice"
    "InputBufferSize"=dword:1000
    "OutputBufferSize"=dword:1000
    "RetryWaitOnError"=dword:3
    "SleepOnNoData"=dword:3E8 
[HKEY_LOCAL_MACHINE\System\CurrentControlSet\GPS Intermediate Driver\Drivers\GPSOnePort]
   "InterfaceType"="COMM"
   "FriendlyName"="QualComm GpsOne Card, version 0.0"
   "CommPort"="COM1:"   
[HKEY_LOCAL_MACHINE\System\CurrentControlSet\GPS Intermediate Driver\Drivers\GPSOneEmulate]
   "InterfaceType"="File"
   "FriendlyName"="QualComm GpsOne File, version 0.0"
   "Filex"="\\windows\\GPSOneFileSimulation.txt"  
[HKEY_LOCAL_MACHINE\System\CurrentControlSet\GPS Intermediate Driver\Drivers\GPSOneDevice]
   "InterfaceType"="POLL"
   "FriendlyName"="QualComm GpsOne Card, version 0.0"
   "DriverName"="TAI"
   "PollInterval"=dword:1F4   
   "Version"=dword:1
 [HKEY_LOCAL_MACHINE\System\CurrentControlSet\GPS Intermediate Driver\Multiplexer]
        "DriverInterface"="COM4:"
[HKEY_LOCAL_MACHINE\System\CurrentControlSet\GPS Intermediate Driver\Multiplexer\ActiveDevice]
   "Dll"="GPSID_QCT.dll"
   "Keep"=dword:1
   "Context"=dword:12344160
[HKEY_LOCAL_MACHINE\SOFTWARE\HTC\SUPL AGPS]
   "EnableAGPS"=dword:00000001   ; 0:Disable AGPS
   "GPSMode"=dword:00000002      ; 1:GPS_FIX_MODE_MSA, 2:GPS_FIX_MODE_MSB, 3:GPS_FIX_MODE_MSS
   "NumberFixes"=dword:3B9AC9FF  ; 999999999
   "TimeBetweenFixes"=dword:00000001   ; 1
   "QoSAccuracy"=dword:00000032        ; 50
   "QosPerformance"=dword:00000059     ; 89
   "ServerIP"="195.207.101.126"  ; Set QCT AGPS Server IP as default
   "ServerPort"=dword:00001E6C   ; Set QCT AGPS Server port as default
   "EnableGPSSmartMode"=dword:00000001   ; Enable GPS smart mode

[HKEY_LOCAL_MACHINE\Software\Microsoft\Shell\Event\Dock\Inbox]
"command"=- ; erase previous default
[HKEY_LOCAL_MACHINE\Comm\ConnMgr\Planner\Settings]
	"SuspendResume"=multi_sz:"#777"
[HKEY_LOCAL_MACHINE\Comm\TcpIp\Parms]
   "TcpWindowSize"=dword:10000
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\SDHC]
    "Order"=dword:21
    "Dll"="sdhc.dll"
    "Prefix"="SDH"
    "ControllerIRQ"=dword:21
    "ControllerISTPriority"=dword:64
    "CardDetectIRQ"=dword:22
    "CardDetectISTPriority"=dword:65
    "ClockAlwaysOn"=dword:0
    "ClockOnIfInterruptsEnabled"=dword:1    
	"IClass"="{8DD679CE-8AB4-43c8-A14A-EA4963FAA715}"   ; power-managed block devices
[HKEY_LOCAL_MACHINE\System\StorageManager\Profiles\SDMemory]
    "Name"="SD Memory Card"
    "Folder"="Storage Card"
[HKEY_LOCAL_MACHINE\System\StorageManager\Profiles\MMC]
    "Name"="MMC Card"
    "Folder"="Storage Card"
[HKEY_LOCAL_MACHINE\Drivers\SDCARD\ClientDrivers\Class\SDMemory_Class]
   "Dll"="SDMemory.dll"
   "Prefix"="DSK"
   "BlockTransferSize"=dword:40  ; send no more than 64 blocks of data per bus transfer
   "Profile"="SDMemory"
   "IClass"=multi_sz:"{A4E7EDDA-E575-4252-9D6B-4195D48BB865}",
                     "{A32942B7-920C-486b-B0E6-92A702A99B35}"
[HKEY_LOCAL_MACHINE\Drivers\SDCARD\ClientDrivers\Class\MMC_Class]
   "Dll"="SDMemory.dll"
   "Prefix"="DSK"
   "BlockTransferSize"=dword:40  ; send no more than 64 blocks of data per bus transfer
   "Profile"="MMC"
   "IClass"=multi_sz:"{A4E7EDDA-E575-4252-9D6B-4195D48BB865}",
                     "{A32942B7-920C-486b-B0E6-92A702A99B35}"   
