Connections Help

# Connect to intranet URLs

If you want to connect to intranet sites that have periods in their URLs (for example, intranet.companyname.com), you must add them to the Work URL Exceptions list.

1. Tap > Settings > Connections tab.
2. Tap Connections > Advanced tab > Exceptions.
3. Tap Add new URL.
4. In Work URL, enter the intranet URL.

Tip

If you use many URLs that share the same root company name, you can avoid entering them individually by entering *.companyname.com.

#### See also

View intranet URLs

Change an intranet URL

# Add a dialing location

1. Tap > Settings > Connections tab.
2. Tap Connections > Advanced tab > Dialing Rules.
3. Tap New.
4. In the Name box, enter a location name, for example, New York.
5. Enter or edit the area code and country code.
6. If you have a pulse phone line, select the Pulse dialing check box. Most phone lines are tone.
7. To automatically disable call waiting, select the Disable call waiting check box. Then, tap the appropriate number sequence in the list, or enter a new sequence.

Tip

To change how the number is dialed, tap Dialing Patterns. For example, enter dialing patterns that will set your device to always dial the number as long distance, or to first dial a 9.

#### See also

Change dialing patterns

Use dialing rules

# Change connection group name

Your device is already set up with two groups of connection settings: My ISP and My Work Network. You can change the name of these groups to something more meaningful for you. For example, if you put all of your corporate settings under My Work Network connections, you can change the name from My Work Network to your company's name.

1. Tap > Settings > Connections tab > Connections.
2. Under My ISP or My Work Network, tap Manage existing connections.
3. Tap the General tab.
4. Enter a name for the settings group.

# Change dialing patterns

The following table lists supported dialing patterns.

To | Enter
Dial a country code | E
Dial an area code | F
Dial a local number | G
Make an international call when using a GSM-network mobile phone, the plus sign is used to indicate that you are about to make an international call (rather than entering the international access number for the country you are in) | + (plus sign)
Insert a pause (typically 2 seconds) | , (comma)
Wait for a credit card tone | $ (dollar sign)
Wait for a second tone (typically used after $) | W
Tone-dial the numbers that follow | T
Pulse-dial the numbers that follow | P
Transfer to another extension (0.5 sec on hook, 0.5 sec off hook) | ! (hookflash)
Wait for a quiet answer (typically indicated by 6.5 seconds of silence followed by a ring tone) | @
Use special controls on some systems (tone only) | ABCD * #

To | Enter
Dial a country code | E
Dial an area code | F
Dial a local number | G
Insert a pause (typically 2 seconds) | , (comma)
Wait for a credit card tone (specified by the dialing program) | $ (dollar sign)
Wait for a second tone (typically used after $) | W
Tone-dial the numbers that follow | T
Pulse-dial the numbers that follow | P
Transfer to another extension (0.5 sec on hook, 0.5 sec off hook) | ! (hookflash)
Wait for a quiet answer (typically indicated by 6.5 seconds of silence followed by a ring tone) | @
Use special controls on some systems (tone only) | ABCD * #

To | Enter
Dial a country code | E
Dial an area code | F
Dial a local number | G
Insert a pause (typically 2 seconds) | , (comma)
Wait for a credit card tone (specified by the dialing program) | $ (dollar sign)
Wait for a second tone (typically used after $) | W
Tone-dial the numbers that follow | T
Pulse-dial the numbers that follow | P
Transfer to another extension (0.5 sec on hook, 0.5 sec off hook) | ! (hookflash)
Wait for a quiet answer (typically indicated by 6.5 seconds of silence followed by a ring tone) | @
Use special controls on some systems (tone only) | ABCD * #

Notes

Hyphens and spaces in dialing strings are ignored.

Some modems may not respond to the above characters even though your device lets you add them to the dial string.

#### See also

Use dialing rules

Add a dialing location

# Change general modem options

- In the Baud rate list, select a new baud rate. For information on the appropriate baud rate for your modem, check the documentation that came with your modem.
- To connect faster when using a modem, clear the Wait for dial tone before dialing check box.
- To pay for calls with a credit card, in the Wait for credit card box, enter the number of seconds you want the device to wait for a credit card prompt, and enter the credit card number in the Extra dial-string modem commands box.
- To save money when connecting, make sure the device does not stay online too long waiting to connect to an ISP or private network. By default, your device will cancel the call if not connected within two minutes. To increase or decrease this wait time, in the Cancel if not connected in box, change the number of seconds.

#### See also

Connect to the Internet

Connect to Work

# Change network card settings

If you use your network card in two locations, such as work and home, you must also change the network to which the network card connects.

1. Tap > Settings > Connections > Network Cards > Network Adapters tab.

   Note that your device may say Wireless Ethernet instead of Network Cards.

2. In the My network card connects to list, select Internet or Work. When connecting to a private network, such as a corporate network at work, select Work. When connecting to your ISP at home, select Internet.

#### See also

Set up a network card

# Change server settings

You should not need to change these settings, unless your server doesn't use dynamically-assigned IP addresses. Most ISPs and private networks use dynamically-assigned IP addresses.

Servers that require an assigned IP address may also require a way to map computer names to IP addresses. Your device supports two name resolutions options: DNS and WINS.

Contact your ISP to determine which name resolution you need to use, obtain the specific server address, and enter the information in the Server tab. Also, ask if alternate addresses are available. An alternate address may enable you to connect when the primary server is unavailable.

#### See also

Connect to the Internet

Connect to Work

# Change an intranet URL

1. Tap > Settings > Connections tab.
2. Tap Connections > Advanced tab > Exceptions.
3. Tap the intranet URL exception you want to change, and make the desired changes.

Tip

To delete a work URL exception, tap and hold it in the list, and tap Delete.

#### See also

View intranet URLs

Connect to intranet URLs

# Configure network security settings

A wireless network can be added either when the network is detected, or manually by entering settings information. Before doing these steps, determine if authentication information is needed.

1. To manually enter information, tap > Settings > Connections tab > Wi-Fi > Wireless tab.

   Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.

2. In Wireless networks, select the network you want to configure.
3. To use authentication, tap the Network Key tab and select the authentication method from the Authentication list.
4. To use data encryption, select an encryption method from the Data encryption list.
5. To automatically use a network key, tap The key is automatically provided. Otherwise, enter the network key.

#### See also

Enter new settings

Set up a wireless network

Configure 802.1x authentication settings

# Configure 802.1x authentication settings

Before doing these steps, determine if authentication information is needed.

1. To manually enter information, tap > Settings > Connections tab > Wi-Fi > Wireless tab.

   Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.

2. In Wireless networks, select the network you want to configure.
3. For increased security, tap 802.1x tab > Use IEEE 802.1x network access control. Then, select the appropriate EAP type.

#### See also

Enter new settings

Configure network security settings

Set up a wireless network

# Select networks

You should not need to change these settings. Contact your ISP or network administrator before attempting to make changes.

Intranet or Ethernet networks are usually used for work-related activities, while Internet networks are used at home to connect to your ISP. The My Work Network settings are used for private network connections, while the Internet settings are used for connecting to Internet addresses.

You can set up programs on your device to use specific connections. For example, you may want your device to connect automatically to your ISP via an Internet network when using Internet Explorer Mobile, but connect to work via a private network when using Messaging.

1. Tap > Settings > Connections tab > Connections > Advanced tab.
2. Tap Select Networks.
3. In the appropriate lists, select My ISP or My Work Network.

#### See also

Connect to Work

Connect to the Internet

# Connect to the Internet

Before you begin, obtain the following information from your Internet service provider (ISP) or wireless service provider: ISP server phone number or access point, user name, and password.

1. Tap > Settings > Connections tab.
2. Do one of the following:
   - Tap Connections, and in My ISP, set up a modem connection.
   - Tap Wi-Fi and set up a network card or a wireless network connection. Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.
3. The connection is started automatically when you begin using a program that requires an Internet connection. For example, when you start Internet Explorer Mobile to browse the Internet, your device connects automatically. To manually start the connection you set up in step 2, do one of the following:
   - In the modem connections list, tap and hold the connection, and tap Connect.
   - On the Wireless tab, tap the connection name, and tap Connect.

Before you begin, obtain the following information from your Internet service provider (ISP) or wireless service provider: ISP server phone number or access point, user name, and password.

1. Tap > Settings > Connections tab.
2. Do one of the following:
   - Tap Connections, and in My ISP, set up a modem connection.
   - Tap Wi-Fi and set up a network card or a wireless network connection. Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.
3. The connection is started automatically when you begin using a program that requires an Internet connection. For example, when you start Internet Explorer Mobile to browse the Internet, your device connects automatically. To manually start the connection you set up in step 2, do one of the following:
   - In the modem connections list, tap and hold the connection, and tap Connect.
   - On the Wireless tab, tap the connection name, and tap Connect.

Before you begin, obtain the following information from your ISP: ISP server phone number or access point, user name, and password.

1. Tap > Settings > Connections tab.
2. Do one of the following:
   - Tap Connections, and in My ISP, set up a modem connection.
   - Tap Wi-Fi and set up a network card or a wireless network connection. Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.
3. To start the connection, insert any necessary equipment into the device, such as a modem card or network (Ethernet) card. The connection is started automatically when you begin using a program that requires an Internet connection. For example, when you start Internet Explorer Mobile to browse the Internet, your device connects automatically. To manually start the connection you set up in step 2, do one of the following:
   - In the modem connections list, tap and hold the connection, and tap Connect.
   - On the Wireless tab, tap the connection name, and tap Connect.

Tips

To set up a network card or wireless network connection to your ISP, add a new connection in Wi-Fi. Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.

To delete a connection, tap and hold the connection you want to remove, and tap Delete.

#### See also

End a connection

Connect to Work

Set up a network card

Set up a wireless network

Set up a modem connection

Set up VPN server connections

Set up proxy server settings

# Connect to Work

Before you begin, obtain the following information from your network administrator: server phone number, user name, and password.

1. Tap > Settings > Connections tab.
2. Do one of the following:
   - Tap Connections, and in My Work Network, set up a modem or VPN server connection.
   - Tap Wi-Fi and set up a network card or a wireless network connection. Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.
3. To start the connection, insert any necessary equipment into the device, such as a modem card or network (Ethernet) card. The connection is started automatically when you begin using a program that requires an Internet connection. For example, when you start Internet Explorer Mobile to browse the Internet, your device connects automatically. To manually start the connection you set up in step 2, do one of the following:
   - In the modem connections list, tap and hold the connection, and tap Connect.
   - On the Wireless tab, tap the connection name, and tap Connect.

1. Tap > Settings > Connections tab.
2. Do one of the following:
   - Tap Connections, and in My Work Network, set up a modem or VPN server connection.
   - Tap Wi-Fi and set up a network card or a wireless network connection. Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.
3. To start the connection, insert any necessary equipment into the device, such as a modem card or network (Ethernet) card. The connection is started automatically when you begin using a program that requires an Internet connection. For example, when you start Internet Explorer Mobile to browse the Internet, your device connects automatically. To manually start the connection you set up in step 2, do one of the following:
   - In the modem connections list, tap and hold the connection, and tap Connect.
   - On the Wireless tab, tap the connection name, and tap Connect.

1. Tap > Settings > Connections tab.
2. Do one of the following:
   - Tap Connections, and in My Work Network, set up a modem or VPN server connection.
   - Tap Wi-Fi and set up a network card or a wireless network connection. Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.
3. To start the connection, insert any necessary equipment into the device, such as a modem card or network (Ethernet) card. The connection is started automatically when you begin using a program that requires an Internet connection. For example, when you start Internet Explorer Mobile to browse the Internet, your device connects automatically. To manually start the connection you set up in step 2, do one of the following:
   - In the modem connections list, tap and hold the connection, and tap Connect.
   - On the Wireless tab, tap the connection name, and tap Connect.

Tip

To delete a connection, tap and hold the connection you want to remove, and tap Delete.

#### See also

End a connection

Set up a network card

Set up a wireless network

Set up a modem connection

Set up VPN server connections

Set up proxy server settings

Connect to the Internet

# End a connection

It can be useful to end a connection when you are done using it. This frees resources on the device and can save connection charges.

- When connected via a modem or VPN, tap on the title bar, and then tap Disconnect.
- When connected via a cable or cradle, detach your device from the cable or cradle.
- When connected via infrared or Bluetooth, move the device away from the other computer or device.
- When connected via a network (Ethernet) card, remove the card from your device.

# Enter new settings

A wireless network can be added either when the network is detected, or manually by entering settings information.

1. To manually enter information, tap > Settings > Connections tab > Wi-Fi > Wireless tab.

   Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.

2. Tap Add New. If the network was detected, tap the network name.
3. In the General tab, enter a network name. If the network was detected, the network name is entered automatically and can't be changed.
4. In Connects to, select what your network connects to, Work or My ISP. To connect directly to another computer instead of a network access point, select the This is a device-to-device (ad-hoc) connection check box.

#### See also

Configure network security settings

Set up a wireless network

Configure 802.1x authentication settings

# Log on to network services

Before you begin, obtain the following information from your network administrator: user name, password, and domain. Some certificates do not require a password.

1. Enter your user name, password, and domain.
2. To save your password so that you will not be prompted each time you connect, select the Save password check box.

Note

Certificates already configured for this network should be automatically selected by your device. If a certificate cannot be automatically selected, you will be prompted to select the necessary certificate.

#### See also

Select a certificate

Configure advanced proxy settings

Set up proxy server settings

# Set up a modem connection

Before you begin, obtain the following information from your Internet service provider (ISP) or wireless service provider: ISP server phone number or access point, user name, and password.

1. Tap > Settings > Connections tab > Connections.
2. To create a new connection, in either My ISP or My Work Network, tap Add a new modem connection, and follow the instructions in the New Connection wizard.
3. Enter a name for the connection, such as your company's name.
4. In the Select a modem list, tap your modem type.

Notes

Wireless connections can be made via a mobile phone network or GPRS. If you are using a mobile phone network to connect, in the Select a modem list, tap Cellular Line. If you are using GPRS, tap Cellular Line (GPRS).

If you are using any type of external modem, in the Select a modem list, select the modem by name. If a listing does not exist for your external modem, tap Hayes Compatible on COM1.

If you call from a business complex or hotel that requires a nine before dialing out, enter 9 in front of the phone number. You can also do this using dialing rules or dialing locations.

If you know that part of the phone number will change frequently as you travel, you can create dialing rules to avoid creating multiple modem connections for the same phone number.

If you are using GPRS, instead of a telephone number you will need to enter the access point name provided by your wireless service provider.

Notes

Wireless connections can be made via a mobile phone network. If you are using a mobile phone network to connect, in the Select a modem list, tap Cellular Line.

If you are using any type of external modem, in the Select a modem list, select the modem by name. If a listing does not exist for your external modem, tap Hayes Compatible on COM1.

If you call from a business complex or hotel that requires a nine before dialing out, enter 9 in front of the phone number. You can also do this using dialing rules or dialing locations.

If you know that part of the phone number will change frequently as you travel, you can create dialing rules to avoid creating multiple modem connections for the same phone number.

Notes

If you are using any type of external modem, in the Select a modem list, select the modem by name. If a listing does not exist for your external modem, tap Hayes Compatible on COM1.

If you call from a business complex or hotel that requires a nine before dialing out, enter 9 in front of the phone number.

#### See also

Change modem connection settings

Use dialing rules

Add a dialing location

Change general modem options

# Configure advanced proxy settings

1. Tap > Settings > Connections tab > Connections.
2. Tap Edit my proxy server. If a proxy server has not been set up, tap Set up my proxy server.
3. Tap Advanced.
4. Select a proxy server type.
5. For the appropriate server type, enter the proxy server name and port.
6. If necessary, enter the credentials for connecting with your proxy server.
7. If you are configuring a Socks proxy, select Socks 4 or Socks 5. If using Socks 5, enter the credentials for connecting with your proxy server.

#### See also

Set up a network card

# Select a certificate

Certificates already configured for this network should be selected automatically by your device. If a certificate cannot be selected automatically, you must select the necessary certificate. For information on the correct certificate to select, see your network administrator.

- To select a certificate, tap the desired certificate. Your device will then connect automatically.

# Set up a wireless network

1. Tap > Settings > Connections tab > Wi-Fi > Wireless tab.

   Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.

2. Do one of the following:
   - If you do not see a desired network, tap Add New and follow the instructions on the screen.
   - Any networks that you have already configured are preferred networks and are listed under Wireless networks. To change network settings, in Wireless networks, tap a network.
3. Under Networks to access, select All available, Only access points or Only computer-to-computer from the list depending on the type of network(s) to which you connect.

Note

On the Wireless tab, tap the connection name, and tap Connect.

#### See also

Enter new settings

Configure network security settings

Configure 802.1x authentication settings

# Set up a network card

Use a network card to connect directly to an Ethernet network. Once connected, you can view the Internet or intranet, or download e-mail. Ensure you purchase and configure a network card that is compatible with your device.

Before you begin, obtain the following information from your network administrator: user name, password, and domain name. Depending on your network, you may need proxy server or VPN connection settings.

1. Insert the network card into your device.
   1. The first time you insert the card, Network Settings will appear automatically so that you can configure the network card. If it does not appear, or to change settings later, tap > Settings > Connections tab > Wi-Fi > Wireless tab.

   Note that your device may say Wireless Ethernet or Network Cards instead of Wi-Fi.

2. To enter specific server information, on the Network Adapters tab, tap the appropriate network adapter, and then tap Name Servers. Most networks use DHCP, so you should not have to change these settings unless you have been instructed to do so.
3. If necessary, connect the network card to the network by using a network cable. For information, see the documentation that came with your network card.
4. To start a connection, insert the network card, and begin using a desired program, such as Internet Explorer Mobile to browse the Internet. Your device will connect automatically.

Note

If you use your network card with two networks, such as a private network at work and one at home for the Internet, you will need to change the network to which the network card connects. For more information, see Change network card settings.

#### See also

Connect to the Internet

Connect to Work

Set up proxy server settings

Set up VPN server connections

# Set up a WAP gateway

To access WAP sites through Internet Explorer Mobile, configure your device to use a WAP gateway. Use the following steps to create a new set of connections to the Internet with WAP gateway settings. Viewing WAP sites is not supported on all devices.

Before you begin, obtain the following information from your ISP: ISP server phone number, user name, and password. Also, contact your wireless service provider and ask for your WAP gateway server name and port number.

1. Tap > Settings > Connections tab > Connections.
2. Tap Edit my proxy server. If a proxy server has not been set up, tap Set up my proxy server.
3. On the Proxy Settings tab, select the This network connects to the Internet and This network uses a proxy server to connect to the Internet check boxes.
4. If necessary, in the Proxy server box, enter the proxy server name.
5. Tap Advanced > WAP.
6. In the Server box, enter the WAP gateway server name. Under Port, enter the port number. The most common WAP port number is 9201.
7. Enter any logon credentials required by the WAP gateway server.

See also

Use dialing rules

Set up a modem connection

Set up a network card

# Change modem connection settings

Before you begin, obtain the following information from your Internet service provider (ISP) or wireless service provider: ISP server phone number or access point, user name, password, domain name, and TCP/IP settings, if needed.

If your device does not have access to a mobile phone network, insert a modem card.

1. Tap > Settings > Connections tab > Connections.
2. In either My ISP or My Work Network, tap Manage existing connections.
3. Select the desired modem connection, tap Edit, and follow the instructions in the connection wizard.
4. To view Help information for any screen in the wizard or while changing settings, tap .

Tips

To manually start a connection, tap and hold the connection, and tap Connect.

To delete a connection, tap and hold the connection you want to remove, and tap Delete.

#### See also

End a connection

Connect to the Internet

Connect to Work

# Set up proxy server settings

If you are connected to your ISP or private network during synchronization, your device should download proper proxy settings during synchronization from your PC. If these settings are not on your PC or need to be changed, ask your ISP or network administrator for the proxy server name, server type, port, type of Socks protocol used, and your user name and password before you begin.

1. Tap > Settings > Connections tab > Connections.
2. If a proxy server has not been set up, tap Set up my proxy server. Otherwise, tap Edit my proxy server, select the desired proxy server, and tap Settings.
3. Select the This network connects to the Internet and This network uses a proxy server to connect to the Internet check boxes.
4. In the Proxy server box, enter the proxy server name.
5. To change such settings as port number or proxy server type, tap Advanced and change desired settings. For more information, see Configure advanced proxy settings.

Tips

To manually start a connection, tap and hold the connection, and tap Connect.

To delete a connection, tap and hold the connection you want to remove, and tap Delete.

#### See also

Connect to Work

Connect to the Internet

# Set up VPN server connections

A VPN connection helps you to securely connect to servers, such as a corporate network, via the Internet. Ask your network administrator for your user name, password, domain name, TCP/IP settings, and host name or IP address of the VPN server before you begin.

1. Tap > Settings > Connections tab > Connections.
2. To create a new VPN server connection, in My Work Network, tap Add a new VPN server connection and follow the instructions in the New Connection wizard.
3. To view additional information for any screen in the wizard or while changing settings, tap .

Tips

To change existing settings, in My Work Network, tap Manage existing connections > VPN tab. Select the desired VPN connection, tap Edit, and follow the instructions on the screen.

To manually start a connection, tap and hold the connection, and tap Connect.

To delete a connection, tap and hold the connection you want to remove, and tap Delete.

You should not need to change any advanced settings. However, you must change advanced settings when:

- The server to which you are connecting does not use dynamically-assigned addresses, and you need to enter your TCP/IP settings.
- You need to change server DNS or WINS settings.

#### See also

End a connection

Connect to Work

Connect to the Internet

# Use dialing rules

Additional numbers may need to be dialed depending on your given location when connecting. For example, if you want to dial from work, a 9 prefix must often be dialed, or an area code is needed.

To avoid creating a new modem connection for every environment, set dialing rules for the locations from which you connect often. Three dialing locations, Home, Mobile, and Work, have been created for you, and you can create more. If a connection cannot be made, your device will give you an opportunity to change the dialing location.

To avoid creating a new modem connection for every environment, set dialing rules for the locations from which you connect often. Three dialing locations, Home, Mobile, and Work, have been created for you, and you can create more. If a connection cannot be made, your device will give you an opportunity to change the dialing location.

To avoid creating a new modem connection for every environment, set dialing rules for the locations from which you connect often. Two dialing locations, Home and Work, have been created for you, and you can create more. If a connection cannot be made, your device will give you an opportunity to change the dialing location.

1. Tap > Settings > Connections tab.
2. Tap Connections > Advanced tab > Dialing Rules.
3. Tap Use dialing rules.
4. Select a location.

Home - Dials the number as a local call without a 9 prefix.

Mobile - Dials the number as a long distance call without the 9 prefix.

Mobile - Dials the number as a long distance call without the 9 prefix.

Work - Dials the number as local call with the 9 prefix.

Tip

To create a new location, tap New and follow the instructions on the screen. To view additional information at any time, tap .

#### See also

Change dialing patterns

# View intranet URLs

Some companies use periods in their intranet URLs (for example, intranet.companyname.com). If you attempt to connect to one of these URLs, Internet Explorer Mobile will search for the Web site in the Internet rather than the company's intranet. To connect to such intranet URLs, they need to be entered as Work URL Exceptions.

To see if your network administrator has already entered your company's intranet URL, do the following:

1. Tap > Settings > Connections tab.
2. Tap Connections > Advanced tab > Exceptions.
3. If you do not see your company's URL listed, tap Add new URL and create a new URL exception. To view additional information while adding the URL, tap .

#### See also

Connect to intranet URLs

Change an intranet URL

# How do I...

Set up a network card

# How do I...

Set up a network card

# How do I...

Set up a network card

# How do I...

Connect to the Internet

Connect to Work

Change connection group name

# How do I...

Set up VPN server connections

Connect to the Internet

Connect to Work

# How do I...

Set up VPN server connections

Connect to the Internet

Connect to Work

# How do I...

Set up VPN server connections

Connect to the Internet

Connect to Work

# How do I...

Connect to Work

Set up VPN server connections

# How do I...

Configure advanced proxy settings

Set up proxy server settings

Set up a WAP gateway

# How do I...

Configure advanced proxy settings

Set up proxy server settings

Set up a WAP gateway

# How do I...

Set up proxy server settings

Configure advanced proxy settings

Set up a WAP gateway

# How do I...

Set up a modem connection

Change modem connection settings

# How do I...

Change server settings

Set up a modem connection

Change modem connection settings

# How do I...

Set up a modem connection

Change modem connection settings

Overview of Terminal Services Client

# How do I...

Set up a modem connection

Change modem connection settings

Change server settings

# How do I...

Set up a modem connection

Change modem connection settings

# How do I...

Set up a modem connection

Change modem connection settings

# How do I...

Set up a modem connection

Change modem connection settings

# How do I...

Set up a modem connection

Change modem connection settings

# How do I...

Change modem connection settings

Set up a modem connection

End a connection

Set up an automatic choice for connections

# How do I...

Change connection group name

Change modem connection settings

Set up a modem connection

# How do I...

Select networks

Connect to Work

Connect to the Internet

# How do I...

Change an intranet URL

View intranet URLs

Connect to intranet URLs

# How do I...

Connect to intranet URLs

Change an intranet URL

View intranet URLs

# How do I...

View intranet URLs

Connect to intranet URLs

Change an intranet URL

# How do I...

Change dialing patterns

Add a dialing location

Use dialing rules

# How do I...

Add a dialing location

Change dialing patterns

Use dialing rules

# How do I...

Use dialing rules

Add a dialing location

Change dialing patterns

# How do I...

Select networks

Use dialing rules

Connect to intranet URLs

View intranet URLs

# How do I...

Connect to the Internet

Connect to Work

End a connection

Set up a WAP gateway

Use dialing rules

View intranet URLs

# How do I...

Log on to network services

Configure advanced proxy settings

# How do I...

Log on to network services

Configure advanced proxy settings

# How do I...

Select a certificate

Configure advanced proxy settings

Configure network security settings

# How do I...

Enter new settings

Set up a wireless network

Configure network security settings

# How do I...

Change server settings

Configure network security settings

Enter new settings

# How do I...

Configure 802.1x authentication settings

Change network card settings

# How do I...

Connect to the Internet

Set up a modem connection

End a connection

# How do I...

Set up a wireless network

Enter new settings

Configure network security settings

# Set up an automatic choice for connections

If you have already created more than one connection, you can set up your device to connect to the best available connection automatically.

1. Tap > Settings > Connections tab > Connections.
2. Under My ISP or My Work Network, tap Manage existing connections.
3. Tap Auto pick.

#### See also

End a connection

Connect to Work

Connect to the Internet

Set up a wireless network

Set up a modem connection

Set up VPN server connections

# Turn wireless power on or off

You can turn the power off to your wireless connections in a single location. This is a quick way to preserve battery power or to prepare your device for an airplane flight.

1. Tap > Settings > Connections tab.
2. Tap Wireless Manager.
3. Do one of the following:
   - Tap the button for a desired wireless connection type (such as Bluetooth or Phone) to turn it off. If it is already turned off, the button is a lighter color and displays an icon marked with an X.
   - Tap All to turn all wireless power on or off (available only when more than one wireless type exists on your device).

Note

To change settings for one of the displayed wireless connection types, tap Menu and tap the type of settings you want to change.

#### See also

Turn on and off Bluetooth

End a Bluetooth partnership

Change phone settings

Change network card settings

# How do I...

Turn wireless power on or off

Turn on and off Bluetooth

End a Bluetooth partnership

Change phone settings

Change network card settings

Overview of Bluetooth virtual COM ports