Previous Topic | | Next Topic

> Dial-up

> In times when you are not within the coverage of a wireless network, use the 1XRTT or EVDO dial-up connection on your device to connect to the Internet or your corporate network. Your device has two groups of connection settings: Sprint and My Work Network. The Sprint settings are used to connect to the Internet, while My Work Network settings can be used to connect to any private or corporate network. Simply fill in the settings and you’ll be ready to start connecting.

> To connect to the Internet via Sprint:

> Use the 1XRTT or EVDO dial-up connection on your device to connect to the Internet. The Sprint PCS connection is preconfigured on your device, which lets you easily access the Internet via the wireless dial-up connection.

> To connect to a private network:

> 1. | Obtain the following information from your network administrator:

> |  | Server phone number.

> |  | User name and password.

> |  | Domain (provided by the network administrator).

> 2. | Tap Start > Settings > Connections tab > Connections.

> 3. | In My Work Network, follow the instructions for each type of connection.

> 4. | Complete the connection wizard, and then tap Finish.

Previous Topic | | Next Topic