REGEDIT4
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\SDHC1]
    "Order"=dword:21
    "Dll"="sdhc1.dll"
    "Prefix"="SDH"
    "ControllerIRQ"=dword:21
    "ControllerISTPriority"=dword:64
    "CardDetectIRQ"=dword:22
    "CardDetectISTPriority"=dword:65
    "ClockAlwaysOn"=dword:0
    "ClockOnIfInterruptsEnabled"=dword:1
    "IClass"="{A32942B7-920C-486b-B0E6-92A702A99B35}"
[HKEY_LOCAL_MACHINE\System\StorageManager\Profiles\SDMemory]
    "Name"="SD Memory Card"
    "Folder"="Storage Card"
[HKEY_LOCAL_MACHINE\System\StorageManager\Profiles\MMC]
    "Name"="MMC Card"
    "Folder"="Storage Card"
[HKEY_LOCAL_MACHINE\Drivers\SDCARD\ClientDrivers\Class\SDMemory_Class]
   "Dll"="SDMemory.dll"
   "Prefix"="DSK"
   "BlockTransferSize"=dword:10  ; send no more than 64 blocks of data per bus transfer
   "Profile"="SDMemory"
    "IClass"=multi_sz:"{A4E7EDDA-E575-4252-9D6B-4195D48BB865}",
                      "{A32942B7-920C-486b-B0E6-92A702A99B35}"
[HKEY_LOCAL_MACHINE\Drivers\SDCARD\ClientDrivers\Class\MMC_Class]
   "Dll"="SDMemory.dll"
   "Prefix"="DSK"
   "BlockTransferSize"=dword:40  ; send no more than 64 blocks of data per bus transfer
   "Profile"="MMC"
   "IClass"=multi_sz:"{A4E7EDDA-E575-4252-9D6B-4195D48BB865}",
                     "{A32942B7-920C-486b-B0E6-92A702A99B35}"
