ClearVue Professional Print Help

Getting Started
Add a Printer
Configure a Printer
Remove a Printer
Setting Print Properties
Supported Printers
Copyright and Trademark
Index

Getting Started

ClearVue Professional products include the Print Components from WESTTEK'S JETCET Print Pocket so that files may be printed from within each ClearVue product. Follow these steps to add and configure printers or to print a file:

1. Make sure device printer connections are enabled. (See manufacturer's manual for steps to enable printer connections.)
2. From ClearVue open the file to print.
3. Select File and then Print.
4. If a printer is not already configured, Configure and Add a Printer.
5. From the Printer drop-down list, select the printer you wish to print to.
6. Select the Print button.
7. Select the Cancel button to exit without printing.

Add a Printer

From Printer drop-down list, select [Configure Printer]. This opens the Add a Printer dialog.

1. Select the Add button to add and Configure a Printer.
2. Select the Set as Default button to set the highlighted printer as your default printer.

Configure a Printer

From the Select Type dialog you have the option to automatically search for a printer to configure or set it up manually.

Automatically Configure a Printer
Manually Configure a Printer

Note: Different types of printers may require unique settings. Refer to the following links for additional information on the following printer connections.

- IrDa Printers
- Network Printers
- Bluetooth Wireless Printers
- IPP Printers (Internet Printing Protocol Printers)

Automatically Configure a Printer

1. From the Select Type window highlight the printer Type and then select Search, or simply select the Search button. This opens a Search box on the bottom of the screen. In this box, a list of printer types is displayed. If you selected a printer type, it will be checked.
2. Check boxes of any printer connection types to find. Uncheck types to exclude from the search.
3. For network printers you also need to configure the network domain (if applicable) by selecting Network from the Settings menu.
4. Select the Start button to begin searching. Printers found are displayed in the top pane with the Remote Name, Description, Type, and Port. (To sort by any of these columns, select Menu and then Sort.)
5. To exit without adding a printer, select Menu and then Exit or select OK without highlighting a printer.
6. Highlight the desired printer from the list and select OK. This opens the Manually Configure a Printer dialog and enters any information collected automatically from the printer.
7. Check the configuration settings for Printer, Model, Printer Name, Port, and Net Path and manually enter any applicable settings that were not automatically populated.
8. Select the Add Printer button.
9. Select Cancel to exit without adding the printer.

Manually Configure a Printer

1. From the Select Type window highlight the printer Type.
2. Select the Next>> button.
3. Select the Printer from the drop-down list.
4. Select the Model from the drop-down list.
5. Enter the Printer Name. This is your nickname for the printer.
6. The default Port for the printer type selected is displayed. This port is usually accepted.
7. Enter the Net Path, if applicable.
8. Select the Add Printer button.
9. Select Cancel to exit without adding the printer.

Remove a Printer

1. From Printer drop-down list, select [Configure Printer]. This opens the Add a Printer dialog.
2. Select the Remove button.
3. Select the OK to remove the printer.
4. Select Cancel to keep the printer and return to the Add a Printer dialog.

Network Printers

To print to a networked printer you must first set up a network card or the wireless network connection (WiFi) on your device.

Automatically Configuring a Network Printer:
- From the Search dialog configure the network domain (if applicable) by selecting Network from the Settings menu.
- When using the Search option JetCet searches the active printer directory for Microsoft Shared Printers. JetCet only supports shared printers.
Manually Configuring a Network Printer:
- In the Manual Printer Configuration dialog enter the network path in the Net Path edit box as \\servername\printer. JetCet currently does not support identifying the printer by ip address.

IrDa Printing

To use the IrDa printing, be sure the IrDa on the device is compatible with the IrDa on the printer. The IrDa's on both devices need to be close together and pointing towards each other.

Bluetooth Wireless Printers

JetCet supports bluetooth printers and adapters using the Serial Port Protocol (SPP). Before you add a Bluetooth printer, set up the Bluetooth connections on your device using the following steps.

1. Enable the Bluetooth radio using the Bluetooth Manager.
2. Bind the printer to your device using the Bluetooth Manager.

When automatically or manually configuring a printer, the Outbound Bluetooth Com Port on your device is automatically populated in the Port field. Changing this field for a Bluetooth printer will cause conflicts during printing and is not recommended.

IPP Printers (Internet Printing Protocol Printers)

- Before you add an IPP printer make sure the printer supports IPP and is configured as an IPP printer.
- IPP printers can only be added manually in JetCet (you can not use the Search option).

To Add an IPP Printer:

1. From the Select Type window highlight IPP Printer then select Next>>.
2. Enter the URL of the IPP printer and then select Add. This will check if the URL is a valid IPP Printer
3. Select the Printer from the drop-down list.
4. Select the Model from the drop-down list.
5. Enter the Printer Name. This is your nickname for the printer.
6. The default Port for the IPP printer is automatically selected.
7. Select the Add Printer button to add the printer.
8. Select Cancel to exit without adding the printer.

Note: After initial ClearVue installation, the Pocket PC must be soft reset in order for IPP to initiate.

Supported Printers

The drivers in JETCET PRINT Pocket conform to these industry standards:

- Hewlett Packard's Printer Control Language (HP-PCL) Version 3
- Epson ESC/P2

For supported printers, please choose one of the following:

- Canon BJC Printers
- Epson Printers
- Hewlett Packard Printers

Canon BJC Printers

Canon BJC 3-Color Printers:
- BJC 1000 and 2000
Canon BJC 4-Color Printers:
- BJC 3000, 4300 and 4400
- BJC 50, 55, 80 and 85
Canon All-Purpose Printers:
- i475D
Canon Photo Printers:
- i560, i860, i960
- i900D
- S600
Canon Mobile Printers:
- i70, i80

Epson Printers

- Stylus C20/C40/C60/C80
- Stylus Color 440/640/670/740/760/777
- Stylus CX3100/CX3200/CX5100/5200
- Stylus Photo 1280/1290/780/790/820/820U/825/830U/875/890/900/915/950/960
- Epson LQ Compatible

Hewlett Packard Printers

- Business Inkjet 2200 Series
- Color LaserJet Series
- CP 1160/1700 Series
- DeskJet: 350, 450, 800C Series, 825/845 Series, 900C Series, 960/980/990C Series, 995C, 1120C Series, 1220C, 3800 and 5500/6100 Series
- LaserJet Monochrome Series
- Office Jet: D Series, G/K/V Series, R/T Series
- PhotoSmart: 100/200 Series, 1000/1100, 1110/1200/1300 Series and 7000 Series
- PSC: 500 Series and 700/900 Series

Setting Print Properties

This option is available for Canon printers only. The Print Properties can be opened by selecting Properties from the Settings dialog in the Configuration window.

The Print Properties Options are:

Quality:

- Color Options:

- Select Color (for color printers only) or Monochrome for the desired print output.
- Under Scheme, select Photo for natural colors print quality, Business Presentation for bright color and Custom for your specific requirements.

- Print Quality:

- High Quality will give better output but will print slower than Normal Quality.

Advanced:

- Toner Saver:

- The default setting "None" gives the highest quality printing and will use the most toner.
- The "Dark" setting uses less toner while still producing the entire image.
- The "Light" setting will print an outline of the letters and uses the least amount of toner.

- Layout Options:

- The Single option produces standard margins while the 2-Up is booklet style.

Index
Add a Printer
Automatically Configure a Printer
Bluetooth Printers
Canon BJC Printers
Configure a Printer
Copyright and Trademark
Epson Printers
Getting Started
Hewlett Packard Printers
IPP Printers
IrDa Printers
Manually Configure a Printer
Network Printers
Remove a Printer
Setting Print Properties
Supported Printers